// BMM LOC annotation file.
//
// Release 12.4 - Data2MEM M.81d, build 1.9 Aug 19, 2010
// Copyright (c) 1995-2014 Xilinx, Inc.  All rights reserved.


///////////////////////////////////////////////////////////////////////////////
//
// Processor 'microblaze_0', ID 100, memory map.
//
///////////////////////////////////////////////////////////////////////////////

ADDRESS_MAP microblaze_0 MICROBLAZE 100


    ///////////////////////////////////////////////////////////////////////////////
    //
    // Processor 'microblaze_0' address space 'lmb_bram_combined' 0x00000000:0x0000FFFF (64 KBytes).
    //
    ///////////////////////////////////////////////////////////////////////////////

    ADDRESS_SPACE lmb_bram_combined RAMB16 [0x00000000:0x0000FFFF]
        BUS_BLOCK
            instance_name/lmb_bram/lmb_bram/ramb16bwer_0 [31:31] INPUT = lmb_bram_combined_0.mem PLACED = X4Y54;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_1 [30:30] INPUT = lmb_bram_combined_1.mem PLACED = X3Y52;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_2 [29:29] INPUT = lmb_bram_combined_2.mem PLACED = X3Y50;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_3 [28:28] INPUT = lmb_bram_combined_3.mem PLACED = X3Y48;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_4 [27:27] INPUT = lmb_bram_combined_4.mem PLACED = X3Y44;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_5 [26:26] INPUT = lmb_bram_combined_5.mem PLACED = X3Y56;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_6 [25:25] INPUT = lmb_bram_combined_6.mem PLACED = X4Y46;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_7 [24:24] INPUT = lmb_bram_combined_7.mem PLACED = X4Y42;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_8 [23:23] INPUT = lmb_bram_combined_8.mem PLACED = X4Y36;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_9 [22:22] INPUT = lmb_bram_combined_9.mem PLACED = X3Y40;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_10 [21:21] INPUT = lmb_bram_combined_10.mem PLACED = X3Y18;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_11 [20:20] INPUT = lmb_bram_combined_11.mem PLACED = X4Y22;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_12 [19:19] INPUT = lmb_bram_combined_12.mem PLACED = X4Y16;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_13 [18:18] INPUT = lmb_bram_combined_13.mem PLACED = X4Y28;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_14 [17:17] INPUT = lmb_bram_combined_14.mem PLACED = X3Y32;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_15 [16:16] INPUT = lmb_bram_combined_15.mem PLACED = X4Y34;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_16 [15:15] INPUT = lmb_bram_combined_16.mem PLACED = X3Y36;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_17 [14:14] INPUT = lmb_bram_combined_17.mem PLACED = X4Y38;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_18 [13:13] INPUT = lmb_bram_combined_18.mem PLACED = X3Y72;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_19 [12:12] INPUT = lmb_bram_combined_19.mem PLACED = X4Y58;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_20 [11:11] INPUT = lmb_bram_combined_20.mem PLACED = X4Y6;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_21 [10:10] INPUT = lmb_bram_combined_21.mem PLACED = X1Y4;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_22 [9:9] INPUT = lmb_bram_combined_22.mem PLACED = X4Y18;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_23 [8:8] INPUT = lmb_bram_combined_23.mem PLACED = X3Y22;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_24 [7:7] INPUT = lmb_bram_combined_24.mem PLACED = X3Y38;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_25 [6:6] INPUT = lmb_bram_combined_25.mem PLACED = X3Y20;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_26 [5:5] INPUT = lmb_bram_combined_26.mem PLACED = X4Y40;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_27 [4:4] INPUT = lmb_bram_combined_27.mem PLACED = X4Y48;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_28 [3:3] INPUT = lmb_bram_combined_28.mem PLACED = X4Y44;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_29 [2:2] INPUT = lmb_bram_combined_29.mem PLACED = X4Y50;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_30 [1:1] INPUT = lmb_bram_combined_30.mem PLACED = X3Y28;
            instance_name/lmb_bram/lmb_bram/ramb16bwer_31 [0:0] INPUT = lmb_bram_combined_31.mem PLACED = X4Y32;
        END_BUS_BLOCK;
    END_ADDRESS_SPACE;

END_ADDRESS_MAP;

