Par Statistics
Total Non-vccgnd Signals= 3079
Total Non-vccgnd Design Pins= 12418
Total Non-vccgnd Conns= 12418
Total Non-vccgnd Timing Constrained Conns= 11547
Phase 1 CPU= 13.8 sec
Phase 2 CPU= 18.0 sec
Phase 3 CPU= 33.1 sec
Phase 4 CPU= 38.5 sec
Phase 5 CPU= 50.0 sec
Phase 6 CPU= 50.0 sec
Phase 7 CPU= 50.0 sec
Phase 8 CPU= 50.0 sec
Phase 9 CPU= 50.0 sec
Phase 10 CPU= 51.5 sec
AvgWirelenPerPin Fanout 1= 5.0
AvgWirelenPerPin Fanout 2= 4.0
AvgWirelenPerPin Fanout 3= 4.0
AvgWirelenPerPin Fanout 4= 6.0
AvgWirelenPerPin Fanout 10= 4.4
AvgWirelenPerPin Fanout 50= 7.8
AvgWirelenPerPin Fanout 100= 7.6
AvgWirelenPerPin Fanout 500= 9.6
AvgWirelenPerPin Fanout 5000= 3.8
AvgWirelenPerPin Fanout 20000= 0.0
AvgWirelenPerPin Fanout 50000= 0.0
AvgWirelenPerPin Fanout 100000= 0.0
IRR Gamma= 1.9103